20130115_SVN138d->SVN145a
1. Enable Cache Read feature for IM-flash
2. Support 256GB for IM-flash
3. Fix FDMA not done hangup issue when ECC fail at NCQ last access LBA
4. Fix free block number inconsistance when ECC fail at Security Erase.
5. Speed up initial timeing when wakeup from DEVSLP
6. Fix ISP mode in DEVSLP HW, set GPIO12 as open-drain.
7. Fix initialize SSD erase count value issue.
----------------------------------------------------------------------------------------
20130117_SVN145a->SVN146a
1.fix can't read thermal sensor valur issue by utility.
2.This package include TSB and Sandisk 256G:
   TH58TEG7DDJTA20_19c_4CH/8CE_TX1H
   TH58TEG8DDJTA20_19c_4CH/4CE_TX3G
   SDTNQGBMB016GP_19c_4CH/8CE_TT1H
 the MPTOOL JMMPTOOL.INI must set "ResPercentage=108"
----------------------------------------------------------------------------------------
20130306_SVN146a->SVN155kw
1. Fix some corner ecc halt FDMA issues;
2. Fix a security erase bug;
3. Fix some SMART attribute content.
4. Enhance the error handling of nand drive 
5. Fix a DevSlp flow bug.
7. Optimization I/M L84A Flash. 
8.This package include TSB and Sandisk 256G:
   TH58TEG7DDJTA20_19c_4CH/8CE_TX1H
   TH58TEG8DDJTA20_19c_4CH/4CE_TX3G
   SDTNQGBMB016GP_19c_4CH/8CE_TT1H
 the MPTOOL JMMPTOOL.INI must set "ResPercentage=108"
----------------------------------------------------------------------------------------
20130403_SVN155kw->SVN167d
1. Enhance L84A NAND error handling.
2. Enhance SATA DEVSLP feature.
3. Integrate TSB19nm TypeC 256GB into standard f/w without over provision.
4.Upgrading F/W from svn155kw to svn167d, must check the "Preformat" option in MPTool.
----------------------------------------------------------------------------------------
20130430_SVN167d->SVN171b
1. Add Intel L84A advanced shift read for higher endurance.
2. Fix some issues of Micron 2 die per 1 ce NAND.
3. Fix the WHCK trim test timeout issue.
4. Fix DRAM test fail by GDP file(02E).
5. Fix Check table file by mp tool(073).
6. Fix SSD have system F/W, Auto detect 2 times issue by mp tool(073).
7. "Test bin" folder only for test use, JM not real verification.
----------------------------------------------------------------------------------------
20130717_SVN171b->SVN198
1. Support L85A Flash at mp tool L85A version.
2. Drive current setting:( just for reference)
    {IM-L85 NAND} 256G:16mA, 128G:14mA, 64G:12mA 
    {SanDisk NAND} 256G:10mA, other: 8mA 
    {SanDisk NAND JM board} 256G: 12mA, other 8mA
3. Add Intel L84A advanced shift read for higher endurance.
4. Fix some issues of Micron 2 die per 1 ce NAND.
5. Fix the WHCK trim test timeout issue.
6. Fix DRAM test fail by GDP file(4/9).
7. Fix Check table file by mp tool(071).
8. 128GB mSATA 1CE2Die partial program.
9. Shorten Shift read delay.
10. Modify Flash error handling for MD5 check issue.(data retention)
11. Add uart_cmd_channel for limiting the dump range and adding a "RWCNT" command to show host R/W info.
12. Flash.ini  modify_130822.
----------------------------------------------------------------------------------------
20131002_SVN198->SVN252
1. This version can't support L85A Flash.
2. Add F/W devslp function on-off switch by ini file.(def.=0, enable=1)
3. Follow JM SMART table to arrange SMART attributes. 
4. Enhance 128GB, 256GB Random Write performance.
5. Pass WHCK8.1 verification.
6. Improve reliability for abnormal power cycle test.
7. Check PCB DEVSLP pin status while Host issues set feature for Device Sleep function but PCB not ready.
8. Improve Code Block protection and reliability.
9. Option items note (base on PCB and Flash):
       If burn in or  temperature test have some ECC error, please try to setting below value:       
       a.Drive current setting by mp tool. (this is controller to Flash current)
       b.Drive current setting by mptool.ini file. (this is Flash to controller)
----------------------------------------------------------------------------------------
20131015_SVN252->SVN263b
1. Fix erase count abnormal under continue abnormal power cycling test.
2. Update mp tool to v101_131107
3. Update GDP to 03939_131107
----------------------------------------------------------------------------------------
20140121_SVN263b->SVN308a
1. enhance NAND ecc fail error handling.
2. Fix COMRESET interrupt NCQ Read/Write command issue.
3. Fix L84A 2die abnormal power cycle fail issue.
4. Support L84C
5. Improve NCQ random Read/write performance.
6. Improve 8CE (TSB 256GB) performance.
7. Improve 32GB, 24GB write performance.
8. Add overdrive 2 for L85A 256GB case.
9. Support L85A 2die


